**Westland Milk Products** **5S Standard**

|  |  |
| --- | --- |
| **Waste Oil Hose – D7 Wetmix** | |
|  | * Clean and sterilise hose inside and out after use and before placing on rack. * No part of the hose should be touching the ground. * Connect cam-lock fittings on each end of the hose. * Ensure the chain is attached to hold hose in place. |